,validTrayDepth##LENGTH##MILLIMETERS,calcOutletPosition##LENGTH##MILLIMETERS,WireGrate##OTHER##,Width_ANZRS##LENGTH##MILLIMETERS,WaveGrate##OTHER##,URL##OTHER##,Type Comments##OTHER##,SillDepth##LENGTH##MILLIMETERS,ProductCode_ANZRS##OTHER##,OutletSizeSelector##OTHER##,OutletSize##LENGTH##MILLIMETERS,OutletPosition##LENGTH##MILLIMETERS,ModifiedIssue_ANZRS##CURRENCY##CURRENCY,Model##OTHER##,Material_ANZRS##OTHER##,Manufacturer##OTHER##,Length_ANZRS##LENGTH##MILLIMETERS,Lateral Flow Rate##PIPING_FLOW##LITERS_PER_SECOND,GrateWidth##LENGTH##MILLIMETERS,GrateMaterial_Wave##OTHER##,GrateMaterial_Solid##OTHER##,GrateMaterial_Perforated##OTHER##,GrateLength##LENGTH##MILLIMETERS,EndBlankThickness##LENGTH##MILLIMETERS,DrainTrayUpperDepth##LENGTH##MILLIMETERS,TrayDepth##LENGTH##MILLIMETERS,DrainDepth##LENGTH##MILLIMETERS,Description##OTHER##,Depth_ANZRS##LENGTH##MILLIMETERS,Default Elevation##LENGTH##MILLIMETERS,CreatedBy_ANZRS##OTHER##,CreatedByURL_ANZRS##OTHER##,Certified_WaterMark##OTHER##,Certified_GlobalGreenTag##OTHER##,CentreOutlet##OTHER##,Calc_ArrayLegs##OTHER##,Assembly Code##OTHER##,AR_WireGrate##OTHER##,65_Range##OTHER##,100_Range##OTHER##,Sitting Angle##OTHER##,Legs##OTHER##
65ARTDi,53,200,1,75,0,https://stormtech.com.au/products/65artdi,,42,65ARTDi,3,50,200,20230914.54,65ARTDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.4,65,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_AR,896,2,25,55,50,"The 65ARTDi is a Threshold Drain for door track with sub sill tray featuring our 65mm wide premium architectural grate. For sliding and Hinged doors. Featuring a linear stainless steel grate with concealed channel section connecting sill and sub-sill for door tracks and thresholds. Allows door sills to be drained while having internal and external floor surfaces with no step down. Please be aware that depending on the installation environment, for a pool installation or close to a surf beach, you may need to have your stainless steel grates electropolished.",95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,1,1,0,1,0
65MNDTDi,53,200,0,75,0,https://stormtech.com.au/products/65mndtdi,,42,65MNDTDi,3,50,200,20230914.54,65MNDTDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.4,65,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_MND,896,2,25,55,50,"The 65MNDTDi is a Threshold Drain for door track with sub sill tray for sliding and hinged doors, featuring our 65mm wide Marc Newson design grate. Featuring a linear stainless steel grate with concealed channel section connecting sill and sub-sill for door tracks and thresholds. Allows door sills to be drained while having internal and external floor surfaces with no step down. Please be aware that depending on the installation environment, for a pool installation or close to a surf beach, you may need to have your stainless steel grates electropolished.",95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,0,1,0,1,0
65PSTDi,53,200,0,75,0,https://stormtech.com.au/products/65pstdi,,42,65PSTDi,3,50,200,20230914.54,65PSTDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.4,65,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_PS,896,2,25,55,50,"The 65PSTDi is a Threshold Drain for door track with sub sill tray for sliding and hinged doors, featuring our 65mm wide Punched Slot grate. Featuring a linear stainless steel grate with concealed channel section connecting sill and sub-sill for door tracks and thresholds. Allows door sills to be drained while having internal and external floor surfaces with no step down. Please be aware that depending on the installation environment, for a pool installation or close to a surf beach, you may need to have your stainless steel grates electropolished.",95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,0,1,0,1,0
65TRTDi,53,200,1,75,0,https://stormtech.com.au/products/65trtdi,,42,65TRTDi,3,50,200,20230914.54,65TRTDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.4,65,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_TR,896,2,25,55,50,"The 65TRTDi is a Threshold Drain for door track with sub sill tray for sliding and hinged doors, featuring our 65mm wide standard grate. Featuring a linear stainless steel grate with concealed channel section connecting sill and sub-sill for door tracks and thresholds. Allows door sills to be drained while having internal and external floor surfaces with no step down. Please be aware that depending on the installation environment, for a pool installation or close to a surf beach, you may need to have your stainless steel grates electropolished.",95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,0,1,0,0,1
100ARTDi,53,200,1,110,0,https://stormtech.com.au/products/100artdi,,42,100ARTDi,5,80,200,20230914.54,100ARTDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.6,100,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_AR,896,2,25,55,50,"The 100ARTDi features our 100mm wide premium architectural style grate. For sliding and Hinged doors. Featuring a linear stainless steel grate with concealed channel section connecting sill and sub-sill for door tracks and thresholds. Allows door sills to be drained while having internal and external floor surfaces with no step down. Please be aware that depending on the installation environment, for a pool installation or close to a surf beach, you may need to have your stainless steel grates electropolished.",95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,1,0,1,1,0
100MNDTDi,53,200,0,110,0,https://stormtech.com.au/products/100mndtdi,,42,100MNDTDi,5,80,200,20230914.54,100MNDTDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.6,100,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_MND,896,2,25,55,50,"The 100MNDTDi is a Threshold Drain for door track with sub sill tray for sliding and hinged doors, featuring our 100mm wide Marc Newson design grate. Featuring a linear stainless steel grate with concealed channel section connecting sill and sub-sill for door tracks and thresholds. Allows door sills to be drained while having internal and external floor surfaces with no step down. Please be aware that depending on the installation environment, for a pool installation or close to a surf beach, you may need to have your stainless steel grates electropolished.",95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,0,0,1,1,0
100PSTDi,53,200,0,110,0,https://stormtech.com.au/products/100pstdi,,42,100PSTDi,5,80,200,20230914.54,100PSTDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.6,100,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_PS,896,2,25,55,50,"The 100PSTDi is a Threshold Drain for door track with sub sill tray for sliding and hinged doors, featuring our 100mm wide Punched Slot grate. Featuring a linear stainless steel grate with concealed channel section connecting sill and sub-sill for door tracks and thresholds. Allows door sills to be drained while having internal and external floor surfaces with no step down. Please be aware that depending on the installation environment, for a pool installation or close to a surf beach, you may need to have your stainless steel grates electropolished.",95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,0,0,1,1,0
100TRTDi,53,200,1,110,0,https://stormtech.com.au/products/100trtdi,,42,100TRTDi,5,80,200,20230914.54,100TRTDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.6,100,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_TR,896,2,25,55,50,"The 100TRTDi is a Threshold Drain for door track with sub sill tray for sliding and hinged doors, featuring our 100mm wide standard grate. Featuring a linear stainless steel grate with concealed channel section connecting sill and sub-sill for door tracks and thresholds. Allows door sills to be drained while having internal and external floor surfaces with no step down. Please be aware that depending on the installation environment, for a pool installation or close to a surf beach, you may need to have your stainless steel grates electropolished.",95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,0,0,1,0,1
100AATDi,53,200,0,110,1,https://stormtech.com.au/products/100artdi,,42,100AATDi,5,80,200,20230914.54,100AATDi Linear Drainage System,Metal_Steel_Stainless_Stormtech_Satin,Stormtech Pty Ltd,900,0.6,100,Grate_Metal_Steel_Stainless_Stormtech_AA,Metal_Steel_Stainless_Stormtech_Satin,Grate_Metal_Steel_Stainless_Stormtech_AR,896,2,25,55,50,The 100AATDi is a Threshold Drain for door track with sub sill tray featuring our 100mm wide Anodised Aluminium Wave grate.,95,1219.2,VinZero Create,https://create.vinzero.com,1,1,0,3,D2030300,0,0,1,1,0
